Feb 24, 2013

Teams 19 & 20: Communications Protocol Specification Document

**Laboratory #2: Requirements and Specification**

**Morgan, Laura Lenig, Tyler**

**Miaw, Jireh Tang, Raymond**

**Hauser, Steven Rupakhetee, Archit**

**Dworak, Catherine McMillion, Andrew**

**Bertoglio, David**

***Work Product***

**This document describes the communication protocol implemented by Teams 19 and 20 for communication between the base station control system, and the robot. This document describes the creation, and decoding process for messages.**

***Document Revision Information***

**2/15/2013 created**

**2/17/2013 designed base station to robot messages**

**2/22/2013 continued design**

**2/24/2013 designed robot to base station messages**

**Approval Sheet**

**All group members whose names are listed below approve of the document and contributed fairly.**

**Member Names**

**Group 19 representative**

**Dworak, Catherine**

**Group 20 representative**

**Lenig, Tyler**

**Pledge**

**On my honor, as a student, I have neither given nor received unauthorized aid on this assignment.**

**Names**

**Group 19**

**Morgan, Laura**

**Miaw, Jireh**

**Hauser, Steven**

**Dworak, Catherine**

**Bertoglio, David**

**Group 20**

**Lenig, Tyler**

**Tang, Raymond**

**Rupakhetee, Archit**

**McMillion, Andrew**

Table of Contents

Introduction 4

About 4

Protocol Description 4

Base Station to Robot Messages 5

Command Structure 5

No-Op 5

Move Straight 5

Move Arc 5

Turn 6

Stop 6

Read Sensor 6

Set Speed 6

Read All Sensors 6

Robot to Base Station Messages 7

Acknowledgment 7

Error Messages 7

Sensor Error Messages 7

Motor Error Messages 7

Sensor Data Messages 7

# Introduction

## About

This document describes the protocol used to communicate between robot and base station system. This protocol allows the base station to control the robot, and allows the robot to send messages including errors to the base station.

## Protocol Description

This protocol uses 10-character messages to communicate between the robot and the base station. These 10-character messages encode both commands from the base station to the robot and messages from the robot to the base station. The messages are structured such that the first two characters determine the type of command or message. The remaining characters are used for various parameters that are documented below.

# Base Station to Robot Messages

## Command Structure

Commands are 10-character messages, where the first two characters are the command type. The remaining characters represent parameters to the command, used by the robot to determine how to execute the command.

### No-Op

**Message:** 0000000000

**Description:** This command is the no operation command can be used to test if messages are being sent. This message is a “null” message.

### Move Straight

**Command Type:** MS

**Parameters:** Forward/Backwards, and distance.

Byte 2 is forward or backwards (F/B)

Bytes 3-9 is distance (#), can be null (0s)

**Description:** This command moves the robot in a straight line. The forward/backward parameter control the direction the robot will move in. The distance allows for the robot to move a specified distance, this parameter can be null. If distance is null, the robot will continually move

**Example Commands:**

MSF0000000 will move the robot forward continuously.

MSB0001000 will move the robot backwards 1000 units.

### Move Arc

**Command Type:** MA

**Parameters:** Forward/Backwards, left/right, radius, distance

Byte 2 is forward or backwards (F/B)

Byte 3 is left or right (L/R)

Byte 4-6 is radius (# degrees)

Byte 7-9 is distance (#), can be null (0s)

**Description:** This command moves the robot in an arc. The forward/backward parameter control the direction the robot will move along the arc. Left/Right will control the direction the robot arcs to. Radius is the absolute value of the number of degrees to move. The distance allows for the robot to move a specified distance, this parameter can be null. If distance is null, the robot will continually move until stopped.

**Example Commands:**

MAFL090000 will move the robot forward to the left along a 90 degree curve continuously

MABR030100 will move the robot backwards along a 30 degree curve for 100 units.

### Turn

**Command Type:** TN

**Parameters:** Left/Right, and radius

Byte 2 is left or right (L/R)

Byte 3-9 is radius (# degrees), can be null (0s)

**Description:** This command turns the robot when stationary. The Left/Right parameter determines the direction the robot turns. The Radius parameter is an absolute value that determines how far the robot turns. If the radius is null, the robot continually turns until stopped.

**Example Commands:**

TNR0000090 will turn the robot right 90 degrees

TNL0000000 will turn the robot left continuously

### Stop

**Message:** ST00000000

**Description:** This command stops any actions that the robot is currently doing. This will end any movement actions.

### Read Sensor

**Command Type:** RS

**Parameters:** Sensor Port

Byte 2 is sensor type (U for Ultrasonic, T for touch, M for sound, L for light)

Bytes 3-9 are 0

**Description:** This command will read a specified sensor. The Sensor Port parameter will determine which sensor to read the value of.

**Example Commands:**

RSU0000000 will cause the robot to read the value of the sensor, and send the data to the base station.

### Set Speed

**Command Type:** SS

**Parameters:** Motor/Motor Combination, and new speed.

Byte 2 is Motor/Motor combination (A for Motor A, B for Motor B, C for Motor C, D for Drive Motors)

Bytes 3-9 is the new speed

**Description:** This command will change the speed of the motors. The combination will determine which motors or combinations of motors to change the speed for.

**Example Commands:**

### Read All Sensors

**Command Message:** RA00000000

**Description:** This command tells the robot to read all sensors and send the data. Each sensor’s data will be sent to the base station in a separate message.

# Robot to Base Station Messages

## Acknowledgment

**Description:** This message is sent to the base station as acknowledgment of receiving a command.

**Message: AK00000000**

## Error Messages

### Sensor Error Messages

**Message Type:** ERS

**Parameters:** Message number

Bytes 3-9 message number

**Description:** This message will tell the base station that an error with a sensor has occurred. The message number maps to a more specific description, that the base station will have stored locally for reference. Available messages can be seen in a table below, which will have additions added as required.

|  |  |
| --- | --- |
| Message Number | Description |
| 0000001 | Error with sensor in port 1 |
| 0000002 | Error with sensor in port 2 |
| 0000003 | Error with sensor in port 3 |
| 0000004 | Error with sensor in port 4 |

### Motor Error Messages

**Message Type:** ERM

**Parameters:** Message Number

Bytes 3-9 message number

**Description:** These messages will tell the base station that an error with a motor has occurred. The message number correlates to a specific description, which the base station has stored locally. Available messages can be seen in a table below, which will have additions added as required.

|  |  |
| --- | --- |
| Message Number | Description |
| 0000001 | Error with motor in port A |
| 0000002 | Error with motor in port B |
| 0000003 | Error with motor in port C |

## Sensor Data Messages

**Message Type:** SD

**Parameters:** Sensor Type, and Data

Byte 2 sensor type (U for Ultrasonic, T for Touch, M for Sound, or L for Light)

Bytes 3-9 sensor data

**Description:** These messages allow for the robot to send data to the base station based on the values of the sensor.